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Prepared for:	Edward Gartner
Recreation Director
Upper Saddle River
376 W Saddle River Rd
Upper Saddle River NJ 07458
usrrecreation@aol.com 		

Operator:	SportCare
Re:		G-Max Testing – Vassar

	Site Information

	Field Name: Lake St-Soccer
	Manufacturer:  n/a

	Field Address: 516 E. Crescent Ave U Saddle River
	Fiber Type:  n/a

	Report Date:  7.23.25
	Average Infill Depth:  36

	Weather: Clear
	Install Date:  n/a

	Test Type:  G-Max Test – 10 locations
	Square Feet:  n/a

	
	Primary Markings: Soccer 



	Report Information

	
G-Max testing was performed on the above-mentioned field.  Testing was performed in accordance with ASTM 1936-10/F355 standards.  Equipment used to perform these tests was a TRIAX 2000 “A” Missile, (calibration certificate available upon request).

Ten (10) drop locations were tested in accordance with ASTM 1936 (see diagram and table).  Triax data acquisition and analysis report drops #1-#30.  Drops were made at ten (10) different field locations.  At each location, three (3) drops were made; the second and third drops at each location were averaged to develop a G-Max value for each drop point.  


	Report Results

	
Referring to the attached test data, the drop locations are numbered 1-10.  The Average column is the G-Max value for that test location (average of drops 2 & 3).

Infill measurements ranged from “34 mm – 37 mm” throughout the field.

The G-Max rating of the field tested in this report ranged from “132 – 154” ASTM 1936/F355 requires a G-Max <200 for safety.  Overall G-Max =140
The field tested in this report has been verified to be in compliance and meets the requirements for play based on the specifications as referenced in ASTM 1936/F355.  The test results reported herein reflect the conditions of the field at the time of testing and at the temperatures reported.


	Report Results

	




[bookmark: _MON_1523872568]	



	




	End A:              
	Pavillion
	End B:
	Townhouses
	Side C:
	Townhouses
	Side D:
	Football




[image: ]



795 East Main Street, Bridgewater, New Jersey 08807
Phone  732-560-8844  Fax  732-560-8580  www.sportcaresfm.com
A CLEAN FIELD …… LOOKS BETTER, PLAYS BETTER, LAST LONGER!
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		Test Location		Drop 1		Drop 2		Drop 3		Average		Gmax Min/Max		Infill Depth (mm)		Infill Min/Max		Field Temp (F)

		9		138		137		142		139.5				36				150

		1		145		136		137		136.5				36				150

		2		144		135		132		133.5				37				150

		3		136		144		138		141				36				150

		4		127		139		146		142.5				35				150

		8		142		158		139		148.5				34				150

		10		154		153		155		154				36				150

		6		145		139		137		138				36				150

		5		148		136		127		131.5				36				150

		7		134		137		136		136.5				35				150

										140		132		36		34

		Date  of Test:  		7.23.25								154				37

		Field Name:		Lake St. Soccer								Name of Tester:						Eric

		General Weather Condition:				Clear						Ambient Air Temp:						93
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Test 

Location Drop 1 Drop 2 Drop 3 Average

Gmax 

Min/Max

Infill 

Depth 

(mm)

Infill 

Min/Max

Field 

Temp (F)

9 138 137 142 139.5 36 150

1 145 136 137 136.5 36 150

2 144 135 132 133.5 37 150

3 136 144 138 141 36 150

4 127 139 146 142.5 35 150

8 142 158 139 148.5 34 150

10 154 153 155 154 36 150

6 145 139 137 138 36 150

5 148 136 127 131.5 36 150

7 134 137 136 136.5 35 150

140 132 36 34

Date  of Test:  7.23.25

154 37

Field Name: Lake St. Soccer Name of Tester: Eric

General Weather Condition:Clear Ambient Air Temp: 93
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