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Prepared for:	Edward Gartner
Recreation Director
Upper Saddle River
376 W Saddle River Rd
Upper Saddle River NJ 07458
usrrecreation@aol.com 		

Operator:	SportCare
Re:		G-Max Testing – Vassar

	Site Information

	Field Name: Lake St-Soccer
	Manufacturer:  n/a

	Field Address: 516 E. Crescent Ave U Saddle River
	Fiber Type:  n/a

	Report Date:  7.23.25
	Average Infill Depth:  36

	Weather: Clear
	Install Date:  n/a

	Test Type:  G-Max Test – 10 locations
	Square Feet:  n/a

	
	Primary Markings: Soccer 



	Report Information

	
G-Max testing was performed on the above-mentioned field.  Testing was performed in accordance with ASTM 1936-10/F355 standards.  Equipment used to perform these tests was a TRIAX 2000 “A” Missile, (calibration certificate available upon request).

Ten (10) drop locations were tested in accordance with ASTM 1936 (see diagram and table).  Triax data acquisition and analysis report drops #1-#30.  Drops were made at ten (10) different field locations.  At each location, three (3) drops were made; the second and third drops at each location were averaged to develop a G-Max value for each drop point.  


	Report Results

	
Referring to the attached test data, the drop locations are numbered 1-10.  The Average column is the G-Max value for that test location (average of drops 2 & 3).

Infill measurements ranged from “34 mm – 37 mm” throughout the field.

The G-Max rating of the field tested in this report ranged from “135 – 160” ASTM 1936/F355 requires a G-Max <200 for safety.  Overall G-Max =145
The field tested in this report has been verified to be in compliance and meets the requirements for play based on the specifications as referenced in ASTM 1936/F355.  The test results reported herein reflect the conditions of the field at the time of testing and at the temperatures reported.


	Report Results
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795 East Main Street, Bridgewater, New Jersey 08807
Phone  732-560-8844  Fax  732-560-8580  www.sportcaresfm.com
A CLEAN FIELD …… LOOKS BETTER, PLAYS BETTER, LAST LONGER!

Microsoft_Excel_Worksheet.xlsx
Sheet1

		Test Location		Drop 1		Drop 2		Drop 3		Average		Gmax Min/Max		Infill Depth (mm)		Infill Min/Max		Field Temp (F)

		9		134		138		142		140				36				150

		1		140		134		135		134.5				35				150

		2		153		143		138		140.5				36				150

		3		143		135		137		136				36				150

		4		137		135		136		135.5				34				150

		8		158		162		158		160				35				150

		6		163		144		158		151				36				150

		10		134		162		139		150.5				37				150

		5		135		144		153		148.5				36				150

		7		146		138		169		153.5				36				150

										145		135		36		34

		Date  of Test:  		7.23.25								160				37

		Field Name:		Lake St. Football								Name of Tester:						Eric

		General Weather Condition:				Clear						Ambient Air Temp:						93
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Test 

Location Drop 1 Drop 2 Drop 3 Average

Gmax 

Min/Max

Infill 

Depth 

(mm)

Infill 

Min/Max

Field 

Temp (F)

9 134 138 142 140 36 150

1 140 134 135 134.5 35 150

2 153 143 138 140.5 36 150

3 143 135 137 136 36 150

4 137 135 136 135.5 34 150

8 158 162 158 160 35 150

6 163 144 158 151 36 150

10 134 162 139 150.5 37 150

5 135 144 153 148.5 36 150

7 146 138 169 153.5 36 150

145 135 36 34

Date  of Test:  7.23.25

160 37

Field Name: Lake St. Football Name of Tester: Eric

General Weather Condition:Clear Ambient Air Temp: 93
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